**G7 Specifikace – Server pro učebny VT**

**min. parametry**

Processor core available: **8, per processor**

Processor cache: 11 MB L3

Processor: Scalable 4110 (8 core, 2.1 GHz, 11 MB, 85W)

**Processor number: 2 processors**

**Processor speed: 2.1 GHz**

Memory type: HPE DDR4 SmartMemory

**Memory: 32 GB (2x 16 GB) RDIMM**

NVDIMM type: NVDIMMs

**Included hard drives: 6 SFF drives -**(300 GB SAS, 10K rpm small form factor hard disk drive in a Smart Carrier)

**Power supply type: 2 HPE 500W Flex Slot Platinum hot-plug power supply kit**

Expansion slots: 2 PCIe 3.0, for detailed descriptions reference the QuickSpecs

Min 3x USB 3.0 Ports

Network controller: **Broadcom 4x 1GbE, optional FlexibleLOM**

Storage controller: Smart Array P408i-a/2 GB plus Smart Storage Battery

System fan features: 5 Hot-plug standard dual rotor redundant fans

Šasi serveru v provedení do racku, rozměr max. 1RU, instalační ližiny musí být součástí dodávky

Max. hloubka: 71 cm

Warranty: 3/3/3