**G7 Specifikace – Server pro učebny VT**

**min. parametry**

Processor core available: **8, per processor**

Processor cache: 11 MB L3

Processor: Scalable 4110 (8 core, 2.1 GHz, 11 MB, 85W)

**Processor number: 2 processors**

**Processor speed: 2.1 GHz**

Memory type: HPE DDR4 SmartMemory

**Memory: 32 GB (2x 16 GB) RDIMM**

NVDIMM type: HPE NVDIMMs

**Included hard drives: 6 SFF drives -**(300 GB SAS, 10K rpm small form factor hard disk drive in a Smart Carrier)

Infrastructure management: Standard: HPE iLO Standard with Intelligent Provisioning (embedded) and HPE OneView Standard (requires download).

**Power supply type: 2 HPE 500W Flex Slot Platinum hot-plug power supply kit**

Expansion slots: 2 PCIe 3.0, for detailed descriptions reference the QuickSpecs

Network controller: **Broadcom 4x 1GbE, optional FlexibleLOM**

Storage controller: HPE Smart Array P408i-a/2 GB plus Smart Storage Battery

System fan features: 5 Hot-plug standard dual rotor redundant fans

Form factor: 1U

Warranty: 3/3/3